BSNL Placement Papers
If the voltage applied across a capacitance is triangular in waveform then the waveform of the current is- 
a) Triangular

b) Trapezoidal

c)) Sinusoidal

d) Rectangular

One of the following statement which is true for relative dielectric constant is -

a) It is dimensionless

b) It is not equal to unity for vacuum

c)) Itâ€™s value for all substances is less than one

d)) None

Pure metals generally have-

a) high conductivity and low temperature coefficient

b) high conductivity and large temperature coefficient

c) low conductivity and zero temperature coefficient

d) low conductivity and high temperature coefficient

For small size, high frequency coils, the most common core material is

a) Air

b) Ferrite

c) Powdered ion

d) Steel

For an abrupt junction Varactor diode, the dependence of device capacitance (C) on applied reverse bias (V) is given by-

a) C a V1/3

b) C a V-1/3 

c) C a V1/2

d) C a V-1/2 

A superconductor is a-

a) A material showing perfect conductivity and Meissner effect below a critical temperature

b) A conductor having zero resistance

c) A perfect conductor with highest dimagnetic susceptibility

d) A perfect conductor which becomes resistive when the current density through it exceeds a critical value

When a semiconductor based temperature transducer has a temperature coefficient of â€“2500 mV/0C then this transducer is indeed a-

a) Thermistor

b) Forward biased pn junction diode

c) Reverse biased pn junction diode 

d) FET

The location of lightning arrestor is -

a) Near the transformer

b) Near the circuit breaker

c) Away from the transformer

d) None

Time constant of an RC circuit increases if the value of the resistance is -

a) Increased

b) Decreased

c) Neither a nor b

d) Both a and b

Intrinsic semiconductors are those which -

a) Are available locally

b) Are made of the semiconductor material in its purest from

c) Have more electrons than holes

d) Have zero energy gaps

The primary control on drain current in a JFET is exerted by -

a) Channel resistance

b) Size of depletion regions

c) Voltage drop across channel

d) Gate reverse bias

The electrical conductivity of metals which is expressed in ohm-1 m-1 is of the order of -

a) 1010

b) 105

c) 10-4

d) 10-6

When biased correctly, a zener diode â€“

a) acts as a fixed resistance

b) has a constant voltage across it

c) has a constant current passing through it

d) never overheats

The current amplification factor adc is given by â€“

a) IC/IE

b) IC/IB 

c) IB/IC

d) IB/IC 

Compared to bipolars, FETs have-

a) high input impedance

b) low input impedance

c) same input impedance

d) none

The source-drain channel of JFET is -

a) ohmic

b) bilateral

c) unilateral

d) both a and b

A diac is equivalent to a -

a) Pair of SCRs

b) Pair of four layer SCRs

c) Diode and two resistors

d) Triac width

When a sample of N type semiconductor has electron density of 6.25 Â´ 1011 /cm3 at 300K and if the intrinsic concentration of carriers in this sample is 2.5 Â´ 1013/cm3 then the hole density will be â€“

a) 106/cm3 

b) 103/ cm3 

c) 1010/ cm3 

d) 1012/ cm3 

When the two networks shown in fig. are equivalent with respect to the terminals 1 and 2 at all frequencies then the values of CA, LB, LC and CC will be â€“



a) 0.5, 0.33, 6, 0.166

b) 0.5, 3, 6, 0.66

c) 0.5, 3, 3, 2

d) 0.5, 3, 6, 0.166

The statement ,In any network of linear impedances, the current flowing at any point is equal to the algebraic sum of the currents caused to flow at that point by each of the sources of emf taken separately with all other emf,s reduced to zeroâ€™ represents -

a) Kirchhoff,s law

b) Norton,s theorem

c) Thevenin,s theorem

d) Superposition theorem

One of the following modes which has the characteristics of attenuation becoming less as the frequency is increased and is attractive at icrowave frequencies of circular cylindrical wave guides is â€“

a) TE1 mode

b) TM01 mode 

c) TE01 mode

d) Higher order mode

A two-port network is symmetrical if â€“

a) z11z22 â€“ z12z21 = 1

b) h11h22 â€“ h12h21 = 1 

c) AD â€“ BC = 1

d) y11y22 â€“ y12y21 = 1

For transmission line load matching over a range of frequencies, it is best to use a-

a) balun

b) broad band directional coupler

c) double stub

d) single stub of adjustable position

The poles and zeros of a driving point function of a network are simple and interlace on the negative real axis with a pole closest to the origin. It can be realised -

a) by an LC network

b) as an RC driving point impedance

c) as an RC driving point admittance

d) only by an RLC network

Poles and zeros of a driving point function of a network are simple and interlace on the jw axis. The network consists of elements â€“

a) R and C

b) L and C

c) R and L

d) R, L and C

For a two port reciprocal network, the output open circuit voltage divided by the input current is equal to â€“

a) B

b) Z12



d) h12

In a short electric doublet the radiation properties are so that-

a) The induction field diminishes as the square root of the distance and is only appreciable in the vicinity of the conductor.

b) In the radiation, magnetic field is minimum when the current is maximum.

c) The radiation resistance of a short doublet antenna is extremely high.

d) Mean rate of power through a unit area of spherical sphere surrounding this doublet is proportional to the square of the elemental length, other factors remaining constant.

The frequency modulated (FM) radio frequency range is nearly -

a) 250 â€“300 MHz

b) 150 â€“ 200 MHz

c) 90 â€“ 105 MHz

d) 30-70 MHz

In an underground cable the distortion in the transmission of carrier frequency can be eliminated by using -

a) Inductive loading

b) Resistive loading

c) Capacitive loading

d) Shielding

The charachteristic impendance of a transmission line with inductance 0.294 mH /m and capacitance 60 pF/m is -

a) 49 W

b) 60 W

c) 70 W

d) 140 W

One of the following statements which is not true for a strip line compared to a waveguide is â€“

a) It can be directly connected to semiconductor microwave devices

b) It is much smaller in size

c) It has a smaller bandwidth

d) Losses are less

For a quarter wavelength ideal transmission line of characteristic impedance 50 ohms and load impedance 100 ohms, the input impedance will be â€“

a) 25W

b) 50W

c) 100W

d) 150W

The depth of penetration or skin depth for an electromagnetic field of frequency â€˜fâ€™ in a conductor of resistivity r and permeability m is-

a) inversely proportional to r and f and directly proportional to m

b) directly proportional to r and inversely proportional to f and m

c) directly proportional to f and inversely proportional to r and m

d) inversely proportional to r and m and directly proportional to f

When an antenna has a gain of 44dB then assuming that the main beam of the antenna is circular in cross-section the beam width will be -

a) 0.4456 0

b) 1.44560

c) 2.44560

d) 3.44560 

Lens antennas used for microwaves are usually made of -

a) Polystyrene

b) Glass of low refractive index

c) Paraboloid surfaces

d) Dielectric media having large refractive index

One of the following types of instrument which is an electrometer is -

a) Electrodynamometer

b) PMMC

c) Electrostatic

d) Moving iron

When an ac current of 5A and dc current of 5A flow simultaneously through a circuit then which of the following statement is true ?

a) An ac ammeter will read less than 10A but more than 5A

b) An ac ammeter will read only 5A

c) A dc ammeter will read 10A

d) A dc ammeter will read zero

When Q factor of a circuit is high, then -

a) power factor of the circuit is high

b) impedance of the circuit is high

c) bandwidth is large

d) none of these

The resolution of a logic analyzerA memoryless system is â€“

a) causal

b) not causal

c) nothing can be said

d) none

An air capacitor is a â€“

a) time variant

b) active device

c) time invariant

d) time invariant and passive device

Thermistors are made of -

a) pure metals

b) pure insulators

c) sintered mixtures of metallic oxides

d) pure semiconductor

Pirani gauge is used to measure â€“

a) very low pressures

b) high pressures

c) pressures in the region of 1 atm

d) fluid flow

These circuits converts input power at one frequency to output power at a different frequency through one stage conversion â€“

a) AC voltage controllers

b) Cyclo converters

c) Phase controlled rectifiers

d) Inverters

In a forward voltage Triggering thyristor changes from â€“

a) off state to on state

b) on state to off state

c) on state to on state

d) off state to off state is -

a) the maximum number of input channels

b) the minimum duration of the glitch it can capture

c) it,s internal clock period

d) the minimum amplitude of input signal it can display

A thyristor, when triggered, will change from forward blocking state to conduction state if its anode to cathode voltage is equal to -

a) peak repetitive off state forward voltage

b) peak working off state forward voltage

c) peak working off state reverse voltage

d) peak non-repetitive off state forward voltage

Gate characteristic of a thyristor-

a) is a straight line passing through origin

b) is of the type Vg = a + bIg

c) is a curve between Vg and Ig

d) has a spread between two curves of Vg â€“ Ig 

A four quadrant operation requires-

a) two full converters in series

b) two full converters connected back to back

c) two full converters connected in parallel

d) two semi converters connected back to back

If for a single phase half bridge inverter, the amplitude of output voltage is Vs and the output power is P, then their corresponding values for a single phase full bridge inverter are â€“

a) Vs, P

b) Vs/2, P

c) 2Vs, 2P

d) 2Vs, P

In an enhancement type MOSFET the output V-I characteristics has â€“

a) only an ohmic region

b) only a saturation region

c) only ohmic region at 10 W voltage value followed by a saturation region at higher voltages

d)an ohmic region at large voltage values preceded by a saturation region at lower voltages

The energy gap in a semiconductor -

a) increases with temperature

b) remains constant

c) slightly increase with temperature

d) decrease with temperature

In an electronic circuit matching means -

a) connecting a high impedance directly to low impedance

b) selection of components which are compatible

c) transferring maximum amount of signal between different kinds of circuits.

d) RC coupled stages

P channel FETs are less superior than N channel FETs because

a) They have higher input impedance

b) They have high switching time

c) They consume less power

d) Mobility of electrons is greater than that of holes

Small increase in temperature in the CE connected transistor is the -

a) Increase in ICEO 

b) Increase in ac current gain

c) Decrease in ac current gain

d) Increase in output resistance

An amplifier has a band width of 20 KHz and a midband gain of 50 without feedback. If a negative feedback of 1% is applied then bandwidth with feedback is -

a) 13. 3 KHz

b) 30KHz

c) 10KHz

d) 40KHz

The output of a class B amplifier -

a) is distortion free

b) consists of positive half cycles only

c) is like the output of a full wave rectifier

d) comprises short duration current pulses

An amplifier with negative feedback -

a) lowers its lower 3 dB frequency

b) raises its upper 3 dB frequency

c) increases its bandwidth

d) all of the above

What changes would be necessary in block C if FM signals are to be received -

a) Block becomes redundant

b) A FM detector would be required

c) A high frequency signal generator

d) An additional local oscillator will be needed

The main disadvantage of Diode-Transistor logic (DTL) is its-

a) greater speed

b) slower speed

c) average speed

d) none of the above

Time delay Dt in digital signals in an SIS O shift register is given by â€“

a) Dt = N Â´ Fc

b) Dt = N Â´ 1/Fc

c) Dt = 1/N Â´ Fc

d) Dt = N Â¸ 1/Fc

The output Qn is 1 in a JK flip flop and it does not change when clock pulse is applied) The possible combination of Jn and Kn can be â€“

(y denotes don't care)

a) y and 0

b) y and 1

c) 0 and y

d) 1 and y

Basic memory cell of dynamic RAM consists of â€“

a) a flip flop

b) a transistor acting as a capacitor

c) a transistor

d) a capacitance

The 2,s complement of 10002 is â€“

a) 0111

b) 0101

c) 1000

d) 0001

According to Barkhausen Criterion Phase shift of signal should be â€“

a) 600

b) 900

c) 1800

d) 3600 

The transmission does not have -

a) Partition noise

b) Flicker noise

c) resistance

d) Short noise

Varoctor diode has non linearity of -

a) capacitance

b) Inductance

c) Resistance

d) Is a linear device

Scattering matrix equation for directional coupler is â€“

a) 

b) 

c) 

d) 

Noise figure is calculated as â€“

a) i/p signal to noise ratio X o/p signal to noise ratio

b) i/p S/N Ratio / O/P S/N Ratio 

c) i/p S/N Ratio / O/P S/N Ratio X 100

d) i/p S/N Ratio + O/P S/N Ratio

You can determine quickly the effect of adding poles and zeros by â€“

a) Nicholas chart

b) Nyquist plot

c) Bode plot

d) Root locus.

The polar plot of G(S) = intercepts real axis at w = wo. Then, the real part and wo are given by-

a) â€“5, 1

b) â€“2.5, 1

c) â€“5,0-5

d) â€“5, 2

The initial and final values of F (t) will be respectively-

a) zero and 1

b) zero and 10

c) 10 and zero

d) 70 and 80

A satellite link uses different frequencies for receiving and transmitting in order to â€“

a) avoid interference from terrestrial microwave links

b) avoid interference between its powerful transmitted signals and weak in coming signal

c) minimize free-space losses

d) maximize antenna gain

The first determining factor in selecting a satellite system is its-

a) EIRP

b) Antenna size

c) Coverage area

d) Antenna gain

Equalizing pulses in TV are sent during-

a) horizontal blanking

b) vertical blanking 

c) the serrations 

d) the horizontal retrace 

The son seems to have -------- from his father a somewhat gloomy and moody manner-

a) washed

b) inherited

c) admired

d) attempt

Essayist works with words as sculptor with-

a) water

b) stone

c) air

d) hills

What is a collection of sheep called ?

a) bunch

b) flock

c) herd

d) comet

Join these sentences meaningfully by choosing the correct alternative from the following :

You can buy a book. You can read it.

a) and

b) nor

c) either

d) neither

What is the opposite of Asperity â€“

a) gentility

b) superiority

c) kindness

d) clarity

The Election Commission functions under-

a) Ministry of Home Affairs

b) Ministry of Law

c) Prime Minister,s Secretariat

d) None of these

Article 352 of Indian Constitution needs to be revoked in case-

a) President,s Rule is to be imposed

b) Emergency is declared

c) Services of a Government servant are to be terminated without any enquiry

d) A political party of national level is to be banned

Radio-activity was first discovered by-

a) Becquerel

b) Madam Curie

c) Rutherford

d) Jenner

Ninth Plan in India ranges from-

a) 1995-2000

b) 1996-2001

c) 1997-2002

d) 1998-2003

How much electricity does India propose to generate through nuclear power by the year 2000 AD?

a) 5,000 MW

b) 10,000 MW

c) 15,000 MW

d) 20,000 MW

In which year did the fall of Bastille take place?

a) 1769

b) 1789

c) 1889

d) 1869

To form a quorum how many members of the Lok Sabha or Rajya Sabha should be present?

a) 1/10th of total membership

b) 1/6th of total membership

c) 1/4th of total membership

d) 1/5th of total membership

How may countries are non-permanent members of the Security Council?

a) 6

b) 7

c) 9

d) 10

The International Date Line is represented by-

a) 1000 meridian

b) 00 meridian

c) 1800 meridian

d) 900 meridian

India,s first satellite was launched from-

a) Sriharikota

b) Cape Kennedy

c) Bangalore

d) A Soviet cosmodrome

Name the author of the famous book "Politics"-

a) Aristotle

b) Socrates

c) Plato

d) None of them

"Guernica" is Picasso,s painting on-

a) The Spanish Civil War

b) The American Civil War

c) The French Revolution

d) The Russian Revolution

The object of the Supreme Court,s Keshvanand Bharati ruling is -

a) To put a limit on Parliament,s amendatory powers

b) To give unlimited powers to Parliament to amend the Constitution

c) To give precedence to Directive Principles over Fundamental Rights

d) None of these

Which country in July ,99 officially announced mastering of indigenously developed neutron bomb technology?

a) N. Korea

b) France

c) India

d) China

Shifting cultivation is commonly used in which of the following states?

a) Tamil Nadu

b) Maharashtra

c) Jammu and Kashmir

d) Nagaland 

